==================================
=    FIRMWARE VERSION HISTORY    =
==================================
=             DB4004             =
==================================
=       DEVA Broadcast Ltd.      =
=  http://www.devabroadcast.com  =
==================================


Version 4.0.2226    (31-May-2024)
==================================
	- Fixed NTP sync issue
	- Fixed Time zone setting issue

Version 3.9.2191    (05-Jan-2024)
==================================
	- Added Frequency offset indicator
	- Improved SNMP Agent

Version 3.8.2172    (01-Sep-2023)
==================================
	- Fixed special characters in settings issue

Version 3.7.1957    (10-Nov-2021)
==================================
	- Added RDS Group counters to SNMP
	- Minor fixes

Version 3.6.1912    (26-Apr-2021)
==================================
	- Fixed RDS character support
	- Fixed GSM modem driver
	- Modified E-mail alarm notification message 
	- Minor fixes

Version 3.5.1857    (08-Sep-2020)
==================================
	- Fixed DEVA Device Manager connection
	- Fixed Audio stream server issue
	- Minor fixes

Version 3.4.1848    (23-Jul-2020)
==================================
	- Improved SMTP encryption support
	- Improved network conectivity
	- Minor fixes

Version 3.3.1829    (04-May-2020)
==================================
	- Fixed RDS RT display issue
	- Fixed GSM Modem settings issue
	- Minor fixes

Version 3.2.1824    (12-Mar-2020)
==================================
	- Fixed regional settings issue
	- Minor fixes

Version 3.1.1768    (11-Oct-2019)
==================================
	- Fixed RDS decoder issue
	- Minor fixes

Version 3.0.1725    (31-May-2019)
==================================
	- Added RDS AF list to SNMP  
	- Minor fixes

Version 2.9.1674    (30-Oct-2018)
==================================
	- Fixed SMS notifications issue
	- Fixed SMTP DEVA test account 
	- Minor fixes

Version 2.8.1573    (06-Nov-2017)
==================================
	- Added Region settings
	- Minor fixes

Version 2.7.1567    (25-Sep-2017)
==================================
	- Fixed Listen button in WEB interface
	- Fixed Tuner frequency change issue

Version 2.6.1550    (18-May-2017)
==================================
	- Maintenance release
	- Fixed MPX output issue

Version 2.4.1493    (21-Nov-2016)
==================================
	- Improved tuner performance

Version 2.3.1481    (16-Sep-2016)
==================================
	- Added Attenuator Auto/DX/Local setting
	- Added SMTP default DEVA account option
	- Added current frequncy information to SNMP alarm traps
	- Fixed RDS BER measurement
	- Minor fixes

Version 2.2.1412    (09-Feb-2016)
==================================
	- Fixed storage issue

Version 2.1.1396    (11-Jan-2016)
==================================
	- Fixed SMTP client issue

Version 2.0.1357    (05-Oct-2015)
==================================
	- Fixed tuner frequency input bug
	- Fixed Logger settings page error
	- Fixed Main page presets buttons bug
	- Minor fixes 

Version 1.9.1284    (23-Jan-2015)
==================================
	- Fixed AES/EBU port issue

Version 1.9.1280    (29-Dec-2014)
==================================
	- Fixed SMTP settings port issue
	- Minor RDS decoding fix

Version 1.9.1230    (08-Sep-2014)
==================================
	- Improved RBDS Call sign support
	- Improved Channel aquisition time control
	- Minor fixes

Version 1.8.1212    (02-Jul-2014)
==================================
	- Fixed Front panel GUI issue
	- Fixed Ethernet and USB communication
	- Minor fixes

Version 1.7.1178    (15-Apr-2014)
==================================
	- Added alarm status information monitoring via SNMP
	- Fixed SNMP table indexing issue
	- Fixed WEB channel editor issue

Version 1.6.1047    (01-Jul-2013)
==================================
	- Added UECP TCP Server for RDS monitoring
	- Added UECP UDP Relay for RDS relay
	- Added new GPO functions - RDS Lock, TA/TP flag indicator 
	- Added "infinite" WEB session functionality
	- Fixed alarms trigger and release timeout setting bug

Version 1.5.1018    (17-Apr-2013)
==================================
	- Extended Network discovery compatibility with DEVA Device Manager
	- Fixed SNMP Trap notifications bug
	- Improved system stability

Version 1.4.1003    (14-Mar-2013)
==================================
	- Improved SMTP client
	- Added Connection Type and Host Name parameters for SMTP client
	- Fixed HTTP port change bug
	- Fixed complex e-mails verification bug
	- Extended SNMP Community strings to 31 chars 
	- WEB Preset buttons automatically update with channel settings change 

Version 1.3.993     (21-Feb-2013)
==================================
 	- Improved system stability
	- Added Stereo mode to Scope in WEB
	- Added used and free storage information in WEB
	- Added storage format button in WEB
	- Improved fan control
	- Moved Clear System Log button from Log tab to Settings->Other, WEB

Version 1.2.965     (19-Dec-2012)
==================================
	- Fixed Bandscan from panel not completing
	- Added ability to monitor RDS parameters with SNMP (Lock, BER, PI, PS, RT, TP, TA, M/S, PTY)  
	- Added ability to monitor Audio Stereo status with SNMP
	- Improved storage stability

Version 1.1.954     (22-Nov-2012)
==================================
	- Improved startup sequence

Version 1.0.925     (06-Nov-2012)
==================================
	- Fixed Signal Quality indicator
	- Fixed IF Bandwidth signal & indicator
	- Removed Network Disable button from WEB
	- Fixed Save&Reboot button in Comm, WEB
	- Added Serial & FW rev in SNMP
	- Improved system log, now with SMS and Call information, Alarms and Login information
	- Implemented WEB Log tab
	- Added System log auto delete interval Parameter
	- Fixed SNMP Settings
	- Fixed DHCP/Static IP Change on the fly
	- Improved Audio Streamer, now up to 256 kbps
	- Fixed Digital Audio Enable/Disable
	- Implemented Audio Loss LED functionality
	- Fixed Factory Default groups
	- Improved log files format
	- Improved MPX Power, now with 60 sec integration and sample every 20 sec
	- Added 200kHz frequency step
	- Changed frequency range from 87-108 to 87.1-108.1
	- Implemented RDS/RBDS mode scales, units and PI/CALL change
	- Fixed empty string apply from panel

Version 0.9.884     (08-Oct-2012)
==================================
	- Initial Release
Known Issues:
	- Digital Audio Enable/Disable not implemented
	- Audio Loss LED functionality not implemented
	- Factory Default Settings ALWAYS resets ALL Settings
	- WEB: Log tab not implemented